{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensions","Unit","","Height","mm","1,680"]
["","","","Width","mm","930"]
["","","","Depth","mm","765"]
["Weight","Unit","","","kg","183.0"]
["Compressor","Type","","","","Hermetically sealed scroll compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-5.0"]
["","","","Max.","°CDB","46.0"]
["","Heating","Ambient","Min.","°CWB","-15.0"]
["","","","Max.","°CWB","15.0"]
["Sound power level","Cooling","","","dBA","78.0"]
["","Heating","","","dBA","78.0"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","22.2"]
["","Piping length","OU - IU","Max.","m","100"]
["","","System","Chargeless","m","30"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Connection pipes","","","","4","4"]
["Power supply","Phase","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","25"]
["Notes","","","","","(1) - Power supply to the FDQ indoor unit is separate"]
["","","","","","(2) - See separate drawings for electrical data"]
["Dimensions","Unit","","Height","mm","","1680"]
["","","","Width","mm","","930"]
["","","","Depth","mm","","765"]
["Weight","Unit","","","kg","","184.0"]
["Compressor","Type","","","","","Hermetically sealed scroll compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-5.0"]
["","","","Max.","°CDB","","46.0"]
["","Heating","Ambient","Min.","°CWB","","-15.0"]
["","","","Max.","°CWB","","15.0"]
["Sound power level","Cooling","","","dBA","","78.0"]
["","Heating","","","dBA","","78.0"]
["Refrigerant","Charge","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Charge","","","tCO2Eq","","19.4"]
["Piping connections","Liquid","","OD","mm","","12.70"]
["","Gas","","OD","mm","","22.2"]
["","Piping length","OU - IU","Max.","m","","100"]
["","","System","Chargeless","m","","30"]
["Power supply","Frequency","","","Hz","","50"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","","25"]