{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZR-MYM"]
[]
[]
[]
[]
["","","","","","RZR48MUYMK"]
["Sound pressure level","Cooling","","Nom.","dBA","50"]
["Refrigerant","GWP","","","","2,087.5"]
["","Charge","","","kg","3.70"]
["","Type","","","","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","52"]
["","","","Min.","°CDB","-5"]
["Piping connections","Level difference","IU - OU","Max.","m","30.0"]
["Dimensions","Unit","","Width","mm","900"]
["","","","Depth","mm","320"]
["","","","Height","mm","1,170"]
["Compressor","Type","","","","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","101"]
["Power supply","Phase","","","","3N~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","380-415/380"]