{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":17,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UATYP-AY1(B)"]
[]
[]
[]
[]
["","","","","","UATYP180AMY1","UATYP240AMY1","UATYP280AMY1","UATYP320AMY1","UATYP450AMY1","UATYP560AMY1","UATYP700AMY1","UATYP850AMY1B8","UATYPC10AMY18","UATYPC10AMY1","UATYPC12AMY18","UATYPC12AMY1"]
["Operation range","Cooling","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46","46","46"]
["","","","Min.","°CDB","20","20","20","20","20","20","20","20","20","20","20","20"]
["Cooling capacity","Nom.","","","kW","16.705 (3)","21.101 (3)","25.790 (3)","29.307 (3)","43,668.000 (3)","55.684 (3)","67.406 (3)","78.6 (3)","101.110 (3)","101.110 (3)","109.609 (3)","109.609 (3)"]
["Heating capacity","Nom.","","","kW","20.222 (3)","22.566 (3)","29.893 (3)","35.755 (3)","46.891 (3)","67.406 (3)","74.733 (3)","87.78 (3)","102.290 (3)","102.290 (3)","126.314 (3)","126.314 (3)"]
["Power input","Cooling","","Nom.","kW","6.860","8.410","10.820","12.840","16.570","21.160","29.200","36.10","43.170","43.170","48.200","48.200"]
["","Heating","","Nom.","kW","6.600","7.540","9.810","11.490","15.710","20.300","26.220","32.10","41.670","41.670","46.800","46.800"]
["EER","","","","","2.44","2.51","2.38","2.28","2.64","2.63","2.31","2.18","2.34","2.34","2.27","2.27"]
["COP","","","","","3.06","2.99","3.05","3.11","2.98","3.32","2.85","2.73","2.45","2.45","2.70","2.70"]
["Evaporator","Supply side","Fan","Nominal ESP","Pa","98","98","98","98","196","196","294","294","294","294","294","294"]
["Evaporator piping connections","Condensation drain size","","OD","mm","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.40","25.4","25.4","25.4","25.4"]
["Condenser","Air flow rate","","Cooling","m³/min","127","160","160","283","320","320","566","","566","566","566","566"]
["","Refrigerant","","GWP","","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9","1,773.9"]
["","","","Charge","tCO2Eq","7.6","9.2","10.6","10.6","8.9","10.3","16.7","17","23.9","23.9","35.5","35.5"]
["","","","Charge","kg","4.3","5.2","6.0","6.0","5.0","5.8","9.4","9.6","13.5, 20.0","13.5, 20.0","20.0","20.0"]
["Dimensions","Unit","","Height","mm","1000","1000","1000","1000","1200","1200","1735","1735","1974","1974","1974","1974"]
["","","","Width","mm","1100","1300","1300","1300","1990","1990","2250","2250","2252","2252","2252","2252"]
["","","","Depth","mm","1530","1530","1530","1530","1800","1800","2800","2800","3180","3180","3180","3180"]
["Weight","Unit","","","kg","","","","","","","","1350","1510","","1600"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3N~","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151."]
["","","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit."]
["","","","","","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle."]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]