{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":20,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UATYQ-CY1"]
[]
[]
[]
[]
["","","","","","UATYQ250MCY18","UATYQ250MCY1","UATYQ250MCY17","UATYQ350MCY17","UATYQ350MCY1","UATYQ450MCY17","UATYQ450MCY18","UATYQ450MCY1","UATYQ550MCY17","UATYQ550MCY1","UATYQ600MCY17","UATYQ600MCY1","UATYQ700MCY17","UATYQ700MCY1","UATYQ900MCY17"]
["Sound pressure level","Cooling","","","dBA","68 (1)","68 (1)","68 (1)","64 (1)","64 (1)","65 (1)","65 (1)","65 (1)","68 (1)","68 (1)","70 (1)","70 (1)","70 (1)","70 (1)","70 (1)"]
["Operation range","Cooling","","Max.","°CDB","","52","","","52","","","52","","52","","52","","52","52"]
["","","","Min.","°CDB","","0","","","0","","","0","","0","","0","","0","0"]
["","Heating","","Max.","°CWB","","18","","","18","","","18","","18","","18","","18","18"]
["","","","Min.","°CWB","","-15","","","-15","","","-15","","-15","","-15","","-15","-15"]
["Evaporator piping connections","Condensation drain size","","OD","mm","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4"]
["Cooling capacity","Nom.","","","kW","27.340 (3)","27.340 (3)","27.340 (3)","35.580 (3)","35.580 (3)","44.720 (3)","44.720 (3)","44.720 (3)","55.690 (3)","55.690 (3)","66.820 (3)","66.820 (3)","72.600 (3)","72.600 (3)","90.000 (3)"]
["Power input","Cooling","","Nom.","kW","8.140","8.140","8.140","10.780","10.780","13.040","13.040","13.040","16.740","16.740","19.650","19.650","21.610","21.610","28.5"]
["","Heating","","Nom.","kW","7.330","","7.330","10.840","","12.860","12.860","","15.540","","18.580","","21.420"]
["Sound power level","Cooling","","","dBA","82","82","82","83","83","83","83","83","87","87","90","90","90","90","90"]
["COP","","","","","3.40","3.40","3.40","3.21","3.21","3.25","3.25","3.25","3.47","3.47","3.32","3.32","3.25","3.25","3.15"]
["Dimensions","Unit","","Width","mm","1,638","1,638","1,638","2,209","2,209","2,209","2,209","2,209","2,209","2,209","2,209","2,209","2,209","2,209","2,209"]
["","","","Depth","mm","2,063","2,063","2,063","2,113","2,113","2,113","2,113","2,113","2,670","2,670","2,670","2,670","2,670","2,670","2,670"]
["","","","Height","mm","1,150","1,150","1,150","1,028","1,028","1,130","1,130","1,130","1,048","1,048","1,302","1,302","1,454","1,454","1,454"]
["Casing","Colour","","","","Light grey","Light grey","Ivory white","Ivory white","Light grey","Ivory white","Light grey","Light grey","Ivory white","Light grey","Ivory white","Light grey","Ivory white","Light grey","Ivory white, Light grey"]
["Weight","Unit","","","kg","445","","","","","","610"]
["EER","","","","","3.36","3.36","3.36","3.30","3.30","3.43","3.43","3.43","3.33","3.33","3.40","3.40","3.36","3.36","3.16"]
["Condenser","Air flow rate","","Cooling","m³/min","","","","","","","","","","","","","","","600.36"]
["","Refrigerant","","Condenser-=-Refrigerant-=-Charge-=-TCO2Eq","TCO2Eq","12.7","12.7","12.7","12.1","12.1","15","15","15","18.2","18.2","21.7","21.7","24.2","24.2","24.2"]
["","","","GWP","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","","","Type","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Heating capacity","Nom.","","","kW","24.910 (3)","24.910 (3)","24.910 (3)","34.790 (3)","34.790 (3)","41.790 (3)","41.790 (3)","41.790 (3)","53.930 (3)","53.930 (3)","61.690 (3)","61.690 (3)","69.610 (3)","69.610 (3)","87.896 (3)"]
["Evaporator","Supply side","Fan","Nominal ESP","Pa","147","147","147","147","147","147","147","147","206","206","206","206","206","206","206"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Name","","","","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151."]
["","","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard","(5) - Sound pressure levels are measured according to JIS B 8616 standard"]
["","","","","","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard","(6) - All performance calculations are strictly according to Eurovent standard"]
["","","","","","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases"]