{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":28,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CYA-DK-R"]
[]
[]
[]
[]
["","","","","CYAL100DK125RB","CYAL100DK125RS","CYAM100DK80RB","CYAM100DK80RS","CYAS100DK80RB","CYAS100DK80RS","CYAL150DK200RB","CYAL150DK200RS","CYAM150DK80RB","CYAM150DK80RS","CYAS150DK80RB","CYAS150DK80RS","CYAL200DK250RB","CYAL200DK250RS","CYAM200DK100RB","CYAM200DK100RS","CYAS200DK100RB","CYAS200DK100RS","CYAL250DK250RB","CYAL250DK250RS","CYAM250DK140RB","CYAM250DK140RS","CYAS250DK140RB","CYAS250DK140RS"]
["Power input","Fan only","Nom.","kW","0.48","0.48","0.27","0.27","0.1426","0.1426","0.7245","0.7245","0.4","0.4","0.2139","0.2139","0.96","0.96","0.53","0.53","0.28","0.28","1.2","1.2","0.67","0.67","0.36","0.36"]
["","Heating","Nom.","kW","0.48","0.48","0.27","0.27","0.1426","0.1426","0.7245","0.7245","0.4","0.4","0.2139","0.2139","0.96","0.96","0.53","0.53","0.28","0.28","1.2","1.2","0.67","0.67","0.36","0.36"]
["Door width","Max.","","m","1","1","1","1","1","1","1.5","1.5","1.5","1.5","1.5","1.5","2","2","2","2","2","2","2.5","2.5","2.5","2.5","2.5","2.5"]
["Door height","Max.","","m","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3","3","3","2.5","2.5","2.3","2.3"]
["Dimensions","Unit","Height","mm","370","370","270","270","270","270","370","370","270","270","270","270","370","370","270","270","270","270","370","370","270","270","270","270"]
["","","Width","mm","1048","1048","1048","1048","1048","1048","1548","1548","1548","1548","1548","1548","2048","2048","2048","2048","2048","2048","2548","2548","2548","2548","2548","2548"]
["","","Depth","mm","745","745","561","561","561","561","745","745","561","561","561","561","745","745","561","561","561","561","745","745","561","561","561","561"]
["Weight","Unit","","kg","83","83","66","66","61","61","141","141","93","93","88","88","155","155","117","117","108","108","196","196","144","144","137","137"]
["Casing","Colour","","","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006"]
["","Material","","","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel"]
["Required ceiling void >","mm","","","520","520","420","420","420","420","520","520","420","420","420","420","520","520","420","420","420","420","520","520","420","420","420","420"]
["Refrigerant","Type","","","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A","R32/R410A"]
["Piping connections","Liquid","OD","mm","9.52","9.52","6.35","6.35","6.35","6.35","9.52","9.52","6.35","6.35","6.35","6.35","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","12.7","12.7","12.7","12.7","19.1","19.1","12.7","12.7","12.7","12.7","19.1","19.1","15.9","15.9","15.9","15.9","19.1","19.1","15.9","15.9","15.9","15.9"]
["Power supply","Power supply-=-Frequency","Frequency","","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Power supply-=-Voltage","Voltage","","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230","230"]