{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB"]
[]
[]
[]
[]
["","","","","","FTXJ25A2V1BB"]
["Power input","Cooling","","Nom.","kW","0.022"]
["","Heating","","Nom.","kW","0.022"]
["Casing","Colour","","","","Black"]
["Dimensions","Unit","","Height","mm","305"]
["","","","Width","mm","900"]
["","","","Depth","mm","212"]
["Weight","Unit","","","kg","12"]
["Fan","Air flow rate","Cooling","High","m³/min","11.4"]
["","","","Medium","m³/min","8.6"]
["","","","Low","m³/min","6"]
["","","","Silent operation","m³/min","4.6"]
["","","Heating","High","m³/min","11.3"]
["","","","Medium","m³/min","9"]
["","","","Low","m³/min","6.4"]
["","","","Silent operation","m³/min","4.6"]
["Sound power level","Cooling","","","dBA","57"]
["Sound pressure level","Cooling","","High","dBA","40"]
["","","","Medium","dBA","33"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","19"]
["","Heating","","High","dBA","40"]
["","","","Medium","dBA","33"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","19"]
["Refrigerant","GWP","","","","675"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.5"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC488A1K"]
["","Wired remote control","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]